**Safety Data Sheets (SDS)**

SECTION 1 **Identification**

**GHS product identifier** Nitrogen, Refrigerated Liquid

**Chemical Name** Nitrogen

**Other means of identification** LIN, Cryogenic Liquid Nitrogen, Liquid Nitrogen,

Liquid Nitrogen NF, Liquid Nitrogen FG

**Product use** Synthetic/Analytical chemistry.

**Synonym** LIN, Cryogenic Liquid Nitrogen, Liquid Nitrogen,

 Liquid Nitrogen NF, Liquid Nitrogen FG

**SDS #** 001188

**Supplier's details** Professional Welding Supply, Inc.

3000 Brittmoore, Bldg B

 Houston, TX 77043

**Phone Number** (713) 690-6888

**EMERGENCY PHONE NUMBER 1 (800) 424-9300**

SECTION 2 **Hazards identification**

**OSHA/HCS Status** This material is considered hazardous by the OSHA Hazard

 Communication Standard (29 CFR 1910.1200).

**Classification of the**

**substance or mixture** GASES UNDER PRESSURE - Refrigerated liquefied gas

**GHS LABEL ELEMENTS**



**Hazard pictograms**

**Signal Word** Warning

**Hazard statements** Contains refrigerated gas; may cause cryogenic burns or

injury. May cause frostbite.

**PRECAUTIONARY STATEMENTS**

**General** Read and follow all Safety Data Sheets (SDS’S) before use. Read label before use. Keep out of reach of children. If medical advice is needed, have product container or

label at hand. Close valve after each use and when empty. Use equipment rated for cylinder pressure. Do not open valve until connected to equipment prepared for use.

Use a back flow preventative device in the piping. Use only equipment of compatible materials of construction. Always keep container in upright position. Do not change or force

fit connections. Avoid spills. Do not walk or roll equipment over spills.

**Prevention** Wear cold insulating gloves and face shield.

Use and store only outdoors or in a well ventilated place.

**Response** Thaw frosted parts with lukewarm water. Do not rub affected area. Get immediate medical attention.

**Storage** Store in a well-ventilated place.

**Disposal** Not applicable.

**Hazards not otherwise**

**classified** Liquid can cause burns similar to frostbite.

SECTION 3 **Composition/information on ingredients**

**Substance/Mixture** Substance

**CHEMICAL NAME** Nitrogen

**Other means of identification** LIN, Cryogenic Liquid Nitrogen, Liquid Nitrogen, Liquid Nitrogen NF, Liquid Nitrogen FG

**CAS number** 7727-37-9

**Product code**  001188

|  |  |  |
| --- | --- | --- |
| **INGREDIENT NAME**NITROGEN, REFRIGERATED LIQUID | **PERCENTAGE**100% | **CAS NUMBER**7727-37-9 |

**There are no additional ingredients present which, within the current knowledge of the supplier and in the concentrations applicable, are classified as hazardous to health or the environment and hence require reporting in this section.**

**Occupational exposure limits, if available, are listed in Section 8.**

SECTION 4 **First aid measures**

**DESCRIPTION OF NECESSARY FIRST AID MEASURES**

**Eye Contact** Immediately flush eyes with plenty of water, occasionally lifting the upper and lower eyelids. Check for and remove any contact lenses. Continue to rinse for at least 10

minutes. Get medical attention if irritation occurs

**Inhalation** Remove victim to fresh air and keep at rest in a position comfortable for breathing. If not breathing, if breathing is irregular or if respiratory arrest occurs, provide artificial

respiration or oxygen by trained personnel. It may be dangerous to the person providing aid to give mouth-to-mouth resuscitation. Get medical attention if adverse health effects persist or are severe. If unconscious, place in recovery position and get medical attention immediately. Maintain an open airway. Loosen tight clothing such as a collar, tie, belt or waistband. In case of inhalation of decomposition products in a fire, symptoms may be delayed. The exposed person may need to be kept under medical surveillance for 48 hours.

**Skin Contact** Wash contaminated skin with soap and water. Remove contaminated clothing and shoes. Get medical attention if symptoms occur. In case of contact with liquid, warm frozen tissues slowly with lukewarm water and get medical attention. Do not rub affected area. Wash clothing before reuse. Clean shoes thoroughly before reuse.

**Ingestion** Remove victim to fresh air and keep at rest in a position comfortable for breathing. Get medical attention if adverse health effects persist or are severe. Ingestion of liquid can

cause burns similar to frostbite. If frostbite occurs, get medical attention. Never give anything by mouth to an unconscious person. If unconscious, place in recovery position and get medical attention immediately. Maintain an open airway. Loosen tight clothing such as a collar, tie, belt or waistband. As this product rapidly becomes a gas when

released, refer to the inhalation section.

**IMPORTANT SYMPTOMS/EFFECTS: ACUTE, DELAYED AND REQUIRED TREATMENT**

**POTENTIAL ACUTE HEALTH EFFECTS**

**Eye Contact** Extremely cold material. Liquid can cause burns similar to frostbite.

**Inhalation** No known significant effects or critical hazards.

**Skin Contact** Extremely cold material. Dermal contact with rapidly evaporating liquid could result in freezing of the tissues or frostbite.

**Frostbite** Try to warm up the frozen tissues and seek medical attention.

**Ingestion** Ingestion of liquid can cause burns similar to frostbite.

**OVER-EXPOSURE SIGNS/SYMPTOMS**

**Eye contact** Adverse symptoms may include frostbite.

**Inhalation** No specific data.

SECTION 5 **Fire-fighting measures**

**EXTINGUISHING MEDIA**

**Suitable extinguishing**

**media** Use an extinguishing agent suitable for the surrounding fire.

**Unsuitable extinguishing**

**media** None known.

**Specific hazards arising**

**from the chemical** Contains gas under pressure. Contains refrigerated gas. In a fire or if heated, a pressure increase will occur and the container may burst or explode.

**Hazardous thermal**

**decomposition products** Decomposition products may include the following materials: nitrogen oxides

**Special protective actions**

**for fire-fighters** Promptly isolate the scene by removing all persons from the vicinity of the incident if there is a fire. No action shall be taken involving any personal risk or without suitable

training. Contact supplier immediately for specialist advice. Move containers from fire area if this can be done without risk. Use water spray to keep fire-exposed containers cool.

**Special protective**

**equipment for fire-fighters** Fire-fighters should wear appropriate protective equipment and self-contained breathing apparatus (SCBA) with a full face-piece operated in positive pressure mode. For incidents involving large quantities, thermally insulated undergarments and thick textile or leather gloves should be worn.

SECTION 6 **Accidental release measures**

**PERSONAL PRECAUTIONS, PROTECTIVE EQUIPMENT AND EMERGENCY PROCEDURES**

**Emergency Procedures for**

**Non-emergency Personnel** No action shall be taken involving any personal risk or without suitable training. Evacuate surrounding areas. Keep unnecessary and unprotected personnel from entering. Do not touch or walk through spilled material. Avoid breathing gas. Provide adequate ventilation. Wear appropriate respirator when ventilation is inadequate. Put on appropriate personal protective equipment.

**Emergency Procedures for**

**Emergency Responders** If specialized clothing is required to deal with the spillage, take note of any information in Section 8 on suitable and unsuitable materials. See also the information in "For nonemergency personnel".

**Environmental precautions** Ensure emergency procedures to deal with accidental gas releases are in place to avoid contamination of the environment. Avoid dispersal of spilled material and runoff and contact with soil, waterways, drains and sewers. Inform the relevant authorities if the product has caused environmental pollution (sewers, waterways, soil or air).

**PROPER METHODS OF CONTAINMENT AND CLEANUP**

**Small Spill** Immediately contact emergency personnel. Stop leak if without risk.

**Large Spill** Immediately contact emergency personnel. Stop leak if without risk. Note: see Section 1 for emergency contact information and Section 13 for waste disposal.

SECTION 7 **Handling and Storage**

**PRECAUTIONS FOR SAFE HANDLING**

**Protective Measures** Put on appropriate personal protective equipment (see Section 8). Contains gas under pressure. Contains refrigerated gas. Do not get in eyes or on skin or clothing. Avoid breathing gas. Empty containers retain product residue and can be hazardous. Do not puncture or incinerate container. Use equipment rated for cylinder pressure. Close

Valve after each use and when empty. Protect cylinders from physical damage; do not drag, roll, slide, or drop. Use a suitable hand truck for cylinder movement. Never allow any unprotected part of the body to touch uninsulated pipes or vessels that contain cryogenic liquids. Prevent entrapment of liquid in closed systems or piping without pressure relief devices. Some materials may become brittle at low temperatures and will easily fracture.

**General Occupational**

**Hygene** Eating, drinking and smoking should be prohibited in areas where this material is handled, stored and processed. Workers should wash hands and face before eating,

drinking and smoking. Remove contaminated clothing and protective equipment before entering eating areas. See also Section 8 for additional information on hygiene measures.

**Conditions for Safe Storage**

**Including any incompatibilities** Store in accordance with local regulations. Store in a segregated and approved area. Store in a dry, cool and well-ventilated area, away from incompatible materials (see

Section 10). Keep container tightly closed and sealed until ready for use. Cylinders should be stored upright, with valve protection cap in place, and firmly secured to prevent falling or being knocked over. Cylinder temperatures should not exceed 52 °C (125 °F).

SECTION 8 **Exposure controls/personal protection**

**CONTROL PARAMETERS/Occupational exposure limits**

|  |  |
| --- | --- |
| **Ingredient name**NITROGEN, REFRIGERATED LIQUID | **Exposure limits**Oxygen Depletion [Asphyxiant] |

**Appropriate engineering**

**Controls** Good general ventilation should be sufficient to control worker exposure to airborne contaminants.

**Environmental exposure**

**Controls** Emissions from ventilation or work process equipment should be checked to ensure they comply with the requirements of environmental protection legislation. In some cases, fume scrubbers, filters or engineering modifications to the process equipment

will be necessary to reduce emissions to acceptable levels.

**INDIVIDUAL PROTECTION MEASURES**

**Hygiene Measures** Wash hands, forearms and face thoroughly after handling chemical products, before eating, smoking and using the lavatory and at the end of the working period. Appropriate techniques should be used to remove potentially contaminated clothing.

Wash contaminated clothing before reusing. Ensure that eyewash stations and safety showers are close to the workstation location.

**Eye/face protection** Safety eyewear complying with an approved standard should be used when a risk assessment indicates this is necessary to avoid exposure to liquid splashes, mists, gases or dusts. If contact is possible, the following protection should be worn, unless the assessment indicates a higher degree of protection: safety glasses with sideshields.

**SKIN PROTECTION**

**Hand protection** Chemical-resistant, impervious gloves complying with an approved standard should be worn at all times when handling chemical products if a risk assessment indicates this is necessary. If contact with the liquid is possible, insulated gloves suitable for low temperatures should be worn. Considering the parameters specified by the glove manufacturer, check during use that the gloves are still retaining their protective properties. It should be noted that the time to breakthrough for any glove material may be different for different glove manufacturers. In the case of mixtures, consisting of several substances, the protection time of the gloves cannot be accurately estimated.

**Body protection** Personal protective equipment for the body should be selected based on the task being performed and the risks involved and should be approved by a specialist before handling this product.

**Other skin protection** Appropriate footwear and any additional skin protection measures should be selected based on the task being performed and the risks involved and should be approved by a specialist before handling this product.

**Respiratory protection** Use a properly fitted, air-purifying or air-fed respirator complying with an approved standard if a risk assessment indicates this is necessary. Respirator selection must be based on known or anticipated exposure levels, the hazards of the product and the safe working limits of the selected respirator.

 .

SECTION 9 **Physical and chemical properties**

**APPEARANCE**

**Physical State** Liquid. [Cryogenic liquid]

**Color** Colorless

**Molecular Weight** 28.01 g/mole

**Molecular Formula** N2

**Boiling/condensation point** -195.8 °C

**Melting/Freezing point** -210°C (-346°F)

**Critical temperature** -146.95°C (-232.5°F)

**Odor** Odorless

**Odor threshold** Not available

**PH** Not available

**Flashpoint** Not available

**Burning time** Not available

**Burning rate** Not available

**Evaporation rate** Not available

**Flammability (solid, gas)** Not available

**Lower and upper explosive**

**(flammable) limits** Not available

**Vapor pressure** Not available

**Vapor density** 0.967 (Air = 1) Liquid Density@BP: 50.46 lb/ft3 (808.3 kg/m3)

**Specific Volume (ft 3/lb)** 13.8889

**Gas density (lb/ft 3)** 0.072

**Relative density** Not available

**Solubility** Not available

**Solubility in water** 0.023 g/l

**Partition coefficient: noctanol/**

**water** 0.67

**Auto-ignition temperature** Not available

**Decomposition temperature** Not available

**SADT** Not available

**Viscosity** Not available

SECTION 10 **Stability and reactivity**

**REACTIVITY** No specific test data related to reactivity available for this product or its ingredients.

**CHEMICAL STABILITY** This chemical is stable.

**POSSIBILITY OF HAZARDOUS**

**REACTIONS** Under normal conditions of storage and use, hazardous reactions will not occur.

**CONDITIONS TO AVOID**  No specific data.

**INCOMPATIBLE MATERIAL** No specific data.

**HAZARDOUS DECOMPOSITION**

**PRODUCTS** Under normal conditions of storage and use, hazardous decomposition products should

not be produced.

**HAZARDOUS POLYMERIZATION** Under normal conditions of storage and use, hazardous polymerization will not occur.

SECTION 11 **Toxicological information**

**TOXICOLOGICAL INFORMATION**

**Acute toxicity** Not available

**Irritation/Corrosion** Not available

**Sensitization** Not available

**Mutagenicity** Not available

**Carcinogenicity** Not available

**Reproductive toxicity** Not available

**Teratogenicity** Not available

**Specific target organ toxicity**

**(single exposure)** Not available

**Specific target organ toxicity**

**(repeated exposure)** Not available

**Aspiration hazard** Not available

**Information on the likely routes**

**of exposure** Not available

**POTENTIAL ACUTE HEALTH EFFECTS**

**Eye contact** Extremely cold material. Liquid can cause burns similar to frostbite.

**Inhalation** No known significant effects or critical hazards.

**Skin contact** Extremely cold material. Dermal contact with rapidly evaporating liquid could result in freezing of the tissues or frostbite.

**Ingestion** Ingestion of liquid can cause burns similar to frostbite.

**SYMPTOMS RELATED TO THE PHYSICAL, CHEMICAL AND TOXICOLOGICAL**

**CHARACTERISTICS**

**Eye Contact** Adverse symptoms may include the following:, frostbite.

**Inhalation** No specific data.

**Skin contact** Adverse symptoms may include the following:, frostbite.

**Ingestion** Adverse symptoms may include the following:, frostbite.

**DELAYED AND IMMEDIATE EFFECTS AND ALSO CHRONIC EFFECTS FROM SHORT**

**AND LONG TERM EXPOSURE**

**Potential immediate effects from**

**short term exposure** Not available

**Potential delayed effects from**

**short term exposure** Not available

**Potential immediate effects from**

**long term exposure** Not available

**Potential delayed effects from**

**long term exposure** Not available

**POTENTIAL CHRONIC HEALTH EFFECTS**

**General** No known significant effects or critical hazards.

**Carcinogenicity** No known significant effects or critical hazards.

**Mutagenicity** No known significant effects or critical hazards.

**Teratogenicity** No known significant effects or critical hazards.

**Developmental effects** No known significant effects or critical hazards.

**Fertility effects** No known significant effects or critical hazards.

**NUMERICAL MEASURES OF TOXICITY**

**Acute toxicity measurements** Not available

SECTION 12 **Ecological information**

**Toxicity** Not available

**Persistence and degradability** Not available

**Bioaccumulative potential**

|  |  |  |  |
| --- | --- | --- | --- |
| **Product/ingredient name**NITROGEN,REFRIGERATED LIQUID | **LogPow**0.67 | **BCF** --- | **Potential**Low |

**Mobility in soil** Not available

**Soil/water partition**

**coefficient (KOC)** Not available

**Other adverse effects** No known significant effects or critical hazards.

SECTION 13 **Disposal considerations**

**DISPOSAL METHODS** The generation of waste should be avoided or minimized wherever possible. Disposal of this product, solutions and any by-products should at all times comply with the requirements of environmental protection and waste disposal legislation and any

regional local authority requirements. Dispose of surplus and non-recyclable products via a licensed waste disposal contractor. Waste should not be disposed of untreated to the sewer unless fully compliant with the requirements of all authorities with jurisdiction.

Empty Professional Welding Supply, Inc.-owned pressure vessels should be returned to Professional Welding Supply, Inc.. Waste packaging should be recycled. Incineration or landfill should only be considered when recycling is not feasible. This material and its container must be disposed of in a safe way. Empty containers or liners may retain some product residues. Do not puncture or incinerate container.

SECTION 14 **Transport information**

**UN Number: UN1977** DOT, TDG, Mexico, IMDG, IATA

**UN proper shipping name:**

**NITROGEN, REFRIGERATED**

**LIQUID** DOT, TDG, Mexico, IMDG, IATA

**Transport hazard class: 2.2** DOT, TDG, Mexico, IMDG, IATA

**Packing group** N/A

**Environment: No** DOT, TDG, Mexico, IMDG, IATA

**ADDITIONAL INFORMATION**

**DOT** limited quantity: Passenger aircraft quantity limitation: 75 kg

 Cargo aircraft quantity limitation: 150 kg

**TDG** Product classified as per the following sections of the

Transportation of Dangerous Goods Regulations: 2.13-2.17 (Class 2).

Explosive limit and limited quantity index 0.125

Passenger carrying road or rail index 75

**IATA** Passenger and cargo aircraft quantity limitation:

50 kg

Cargo aircraft only quantity limitation: 500 kg

**“Refer to CFR 49 (or authority having jurisdiction) to determine the information required for shipment of the product.”**

**Special precautions for user** Transport within user’s premises**:** always transport in closed containers that are upright and secure. Ensure that persons transporting the product know what to do in the event of an accident or spillage.

**Transport within user’s premises** Not available

SECTION 15 **Regulatory information**

**U.S. Federal regulations** TSCA 8(a) CDR Exempt/Partial exemption: This material is listed or exempted.

United States inventory (TSCA 8b): This material is listed or exempted.

**Clean Air Act Section 112**

**(b) Hazardous Air**

**Pollutants (HAPs)** Not listed

**Clean Air Act Section 602**

**Class I Substances** Not listed

**Clean Air Act Section 602**

**Class II Substances** Not listed

**DEA List I Chemicals**

**(Precursor Chemicals)** Not listed

**DEA List II Chemicals**

**(Essential Chemicals)** Not listed

**SARA 302/304**

**Composition/information on**

**Ingredients** No products were found.

**SARA 304 RQ** Not applicable

**SARA 311/312**

**Classification** Sudden release of pressure

**COMPOSITON/INFORMATION ON NITROGEN, REFRIGERATED**

**LIQUID INGREDIENTS**

**Percentage** 100%

**Fire hazard** No

**Sudden release of pressure** Yes

**Reactive** No

**Immediate health hazard** No

**Delayed health hazard** No

**STATE REGULATIONS**

**Massachusetts** This material is listed.

**New York** This material is not listed**.**

**New Jersey** This material is listed**.**

**Pennsylvania** This material is listed**.**

**INTERNATIONAL REGULATIONS**

**Australia** This material is listed or exempted.

**Canada** This material is listed or exempted.

**China** This material is listed or exempted.

**Europe** This material is listed or exempted.

**Japan** Not determined.

**Republic of Korea** This material is listed or exempted.

**Malaysia** Not determined.

**New Zealand** This material is listed or exempted.

**Philippines** This material is listed or exempted.

**Taiwan** Not determined.

**Canada** **WHMIS**  Class A: Compressed gas.

**CEPA Toxic substances** This material is not listed.

**Canadian ARET** This material is not listed.

**Canadian NPRI** This material is not listed.

**Alberta Designated Substances** This material is not listed.

**Ontario Designated Substances** This material is not listed.

**Quebec Designated Substances** This material is not listed.

SECTION 16 **Other information**

**Canada label requirements**  Class A: Compressed gas

**HAZARDOUS MATERIAL INFORMATION SYSTEM (U.S.A.)**



3

0

2

**Caution: HMIS® ratings are based on a 0-4 rating scale, with 0 representing minimal hazards or risks, and 4 representing significant hazards or risks Although HMIS® ratings are not required on SDSs under 29 CFR 1910. 1200, the preparer may choose to provide them. HMIS® ratings are to be used with a fully implemented HMIS®**

**program. HMIS® is a registered mark of the National Paint & Coatings Association (NPCA). HMIS® materials may be purchased exclusively from J. J. Keller**

**(800) 327-6868.**

**The customer is responsible for determining the PPE code for this material.**

**NATIONAL FIRE PROTECTION ASSOCIATION (U.S.A.)**



**Reprinted with permission from NFPA 704-2001, Identification of the Hazards of Materials for Emergency Response Copyright ©1997, National Fire Protection Association, Quincy, MA 02269. This reprinted material is not the complete and official position of the National Fire Protection Association, on the referenced subject**

**which is represented only by the standard in its entirety.**

**Copyright ©2001, National Fire Protection Association, Quincy, MA 02269. This warning system is intended to be interpreted and applied only by properly trained individuals to identify fire, health and reactivity hazards of chemicals. The user is referred to certain limited number of chemicals with recommended classifications in NFPA 49 and NFPA 325, which would be used as a guideline only. Whether the chemicals are classified by NFPA or not, anyone using the 704 systems to classify chemicals does so at their own risk.**

**PROCEDURE USED TO DERIVE THE CLASSIFICATION**

|  |  |
| --- | --- |
| **Classification** Press. Gas Refr. Liq. Gas, H281 | **Justification**Expert Judgment |

**To the best of our knowledge, the information contained herein is accurate. However, neither the above-named supplier, nor any of its subsidiaries, assumes any liability whatsoever for the accuracy or completeness of the information contained herein.**

**Final determination of suitability of any material is the sole responsibility of the user. All materials may present unknown hazards and should be used with caution. Although certain hazards are described herein, we cannot guarantee that these are the only hazards that exist.**